**SCHEDULE 1**

**Section 1: Technical Characteristics of Participating Generator Units**

Entity Name

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Resource Name(Generating Unit) | CAISO Resource ID | Type Of Unit | Primary Fuel Type | Resource  Maximum Operating Value 1,2  (PMax MW) | Resource  Minimum Operating Value 1,3  (PMin MW) | Hybrid (Y/N) | Co-Located (Y/N) | ACC ID / ACC Limits (*if unit is Co-Located*)  Maximum & Minimum Operating Value *must* be provided if Co-Located | Net capacity to the CAISO Controlled (MW) | Limitations (That affect technical characteristics and performance of the unit - include those not captured in the GRDT) |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |
| 1. Current effective values for purposes of submitting Self-Schedules and Bids for Energy and/or Ancillary Services in the CAISO Markets may differ from those set forth in this Schedule 1, depending on the results of CAISO performance testing pursuant to Sections 8.9, 8.10 and Appendix K: Ancillary Services Requirements Protocol of the CAISO Tariff. This and other values are subject to certification by the CAISO in accordance with Section 4.3.2 of the Participating Generator Agreement and the CAISO Tariff. More detailed Generating Unit operating data must be provided at a time and in a format specified by the CAISO in response to CAISO requests pursuant to CAISO Tariff Sections 4.6.4 and 4.6.7.1 and 30. 2. The maximum allowable capability when the resource is operating. 3. The maximum allowable charging level when the resource is operating, if applicable. The value will be 0 for non-storage generating type. | | | | | | | | | | |

**SCHEDULE 1**

**Section 2: Limitations**

Entity Name

|  |  |
| --- | --- |
| Resource ID | Description Limitation |
|  |  |