DP 8.7.2	Operating Reserve
(a)	Spinning Reserve:
(i) 	Spinning Reserve provided from Generating Units and Interconnection schedules must meet the standards specified in the ASRP;
(ii)	the ISO will dispatch Spinning Reserve as may be required to meet the Applicable Reliability Criteria;
(iii)	the ISO may dispatch Spinning Reserve as balancing Energy to return Regulation Generating Units to their Set Points and restore full Regulation margin; and
(iv)	the ISO will dispatch Spinning Reserve in merit order of Energy bid prices as determined by BEEP;
(b)	Non-Spinning Reserve:
(i)	Non-Spinning Reserve provided from Generating Units, Demands, and external imports of System Resources must meet the standards specified in the ASRP;
(ii)	the ISO may dispatch Non-Spinning Reserve in place of Spinning Reserve to meet Applicable Reliability Criteria;
(iii)	the ISO will dispatch Non-Spinning Reserve in merit order of Energy bid prices as determined by BEEP; and
(iv)	the ISO may dispatch Non-Spinning Reserve to replace Spinning Reserve if there is a shortfall in Spinning Reserve because of a deficiency of balancing Energy;

DP 9.1.1	Range of ISOAuthority
The ISO has full authority to:
(a)	direct the physical operation of the ISO Controlled Grid,Iincluding (without limitation) circuit breakers, switches, voltage control equipment, protective relays, metering and Load Shedding equipment;
(b)	commit Reliability Must-Run Generation;
(c)	order a change in operating status of voltage control equipment; 
(d)	take required action to prevent against uncontrolled losses of load or Generation;
(e)	control the output of Generating Units and Interconnection schedules scheduled to provide Ancillary Services or offering Supplemental Energy;
(f)	dispatch Curtailable Demand which has been scheduled to provide Non-Spinning Reserve or Replacement Reserve; and
(g)	require the operation of resources which are at the ISO’s disposal in a System Emergency, as described in DP 10.