***\*\*\*The CAISO’s January 2021 filing with include the following proposed tariff revisions. The CAISO will post the remainder of the revised tariff revisions, based on stakeholder comments, in the first quarter of 2021 for a Fall implementation.\*\*\****

**Hybrid Resource**

A Mixed-fuel Resource with a single Resource ID at a single Point of Interconnection.

**Mixed-fuel Resource**

A Generating Facility with components that use different fuel sources or technologies, participating as a Hybrid Resource or Co-located Resources.

…

**34.13.3 Co-located Resources and Dispatch Instructions**

Co-located Resources that are Non-Generator Resources may deviate from Dispatch Instructions only pursuant to this Section. A Co-located Resource that is a Non-Generator Resource may deviate from a Dispatch Instruction where a co-located Eligible Intermittent Resource at the same Generating Facility is producing above its Dispatch Operating Target due to meteorological conditions such that the Co-located Resources’ combined output would exceed the Interconnection Service Capacity of the Co-located Resources, or otherwise threaten reliability or safety. Such deviations may only occur through proper control technologies that ensure the combined output of all Co-located Resources does not exceed the Generating Facility’s Interconnection Service Capacity, .

All deviations from Dispatch Instruction will be subject to Uninstructed Imbalance Energy. A Co-located Resource that is a Non-Generator Resource may not deviate from a Dispatch Instruction pursuant to this section if it is providing Ancillary Services in the same Dispatch Interval.

\* \* \*